From a768af05b1ffe644f54303036e5c048952e0f721 Mon Sep 17 00:00:00 2001
From: Madalin Bucur <madalin.bucur@freescale.com>
Date: Mon, 4 Apr 2016 20:23:21 +0300
Subject: [PATCH 65/70] dpaa_eth: replace sgmii-2500 with qsgmii

Signed-off-by: Madalin Bucur <madalin.bucur@freescale.com>
---
 drivers/net/ethernet/freescale/sdk_dpaa/mac.c |    6 ------
 1 file changed, 6 deletions(-)

--- a/drivers/net/ethernet/freescale/sdk_dpaa/mac.c
+++ b/drivers/net/ethernet/freescale/sdk_dpaa/mac.c
@@ -74,7 +74,6 @@ static const char phy_str[][11] = {
 	[PHY_INTERFACE_MODE_RGMII_TXID]	= "rgmii-txid",
 	[PHY_INTERFACE_MODE_RTBI]	= "rtbi",
 	[PHY_INTERFACE_MODE_XGMII]	= "xgmii",
-	[PHY_INTERFACE_MODE_QSGMII]	= "sgmii-2500"
 };
 
 static phy_interface_t __pure __attribute__((nonnull)) str2phy(const char *str)
@@ -101,7 +100,6 @@ static const uint16_t phy2speed[] = {
 	[PHY_INTERFACE_MODE_RGMII_TXID]	= SPEED_1000,
 	[PHY_INTERFACE_MODE_RTBI]	= SPEED_1000,
 	[PHY_INTERFACE_MODE_XGMII]	= SPEED_10000,
-	[PHY_INTERFACE_MODE_QSGMII]	= SPEED_2500
 };
 
 static struct mac_device * __cold
@@ -341,10 +339,6 @@ static int __cold mac_probe(struct platf
 		mac_dev->if_support &= ~(SUPPORTED_10baseT_Half |
 					SUPPORTED_100baseT_Half);
 
-	if (strstr(char_prop, "sgmii-2500"))
-		mac_dev->if_support &= ~(SUPPORTED_10baseT_Half |
-					SUPPORTED_100baseT_Half);
-
 	/* Gigabit support (no half-duplex) */
 	if (mac_dev->max_speed == SPEED_1000 ||
 	    mac_dev->max_speed == SPEED_2500)
