From 6a6c067b7ce2b3de4efbafddc134afbea3ddc1a3 Mon Sep 17 00:00:00 2001
From: Matthew McClintock <mmcclint@codeaurora.org>
Date: Fri, 8 Apr 2016 15:26:10 -0500
Subject: [PATCH] qcom: ipq4019: use v2 of the kpss bringup mechanism

v1 was the incorrect choice here and sometimes the board
would not come up properly.

Signed-off-by: Matthew McClintock <mmcclint@codeaurora.org>
Signed-off-by: Christian Lamparter <chunkeey@gmail.com>
---
Changes:
	- moved L2-Cache to be a subnode of cpu0
---
 arch/arm/boot/dts/qcom-ipq4019.dtsi | 32 ++++++++++++++++++++++++--------
 1 file changed, 24 insertions(+), 8 deletions(-)

--- a/arch/arm/boot/dts/qcom-ipq4019.dtsi
+++ b/arch/arm/boot/dts/qcom-ipq4019.dtsi
@@ -35,19 +35,27 @@
 		cpu@0 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a7";
-			enable-method = "qcom,kpss-acc-v1";
+			enable-method = "qcom,kpss-acc-v2";
+			next-level-cache = <&L2>;
 			qcom,acc = <&acc0>;
 			qcom,saw = <&saw0>;
 			reg = <0x0>;
 			clocks = <&gcc GCC_APPS_CLK_SRC>;
 			clock-frequency = <0>;
 			operating-points-v2 = <&cpu0_opp_table>;
+
+			L2: l2-cache {
+				compatible = "qcom,arch-cache";
+				cache-level = <2>;
+				qcom,saw = <&saw_l2>;
+			};
 		};
 
 		cpu@1 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a7";
-			enable-method = "qcom,kpss-acc-v1";
+			enable-method = "qcom,kpss-acc-v2";
+			next-level-cache = <&L2>;
 			qcom,acc = <&acc1>;
 			qcom,saw = <&saw1>;
 			reg = <0x1>;
@@ -59,7 +67,8 @@
 		cpu@2 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a7";
-			enable-method = "qcom,kpss-acc-v1";
+			enable-method = "qcom,kpss-acc-v2";
+			next-level-cache = <&L2>;
 			qcom,acc = <&acc2>;
 			qcom,saw = <&saw2>;
 			reg = <0x2>;
@@ -71,7 +80,8 @@
 		cpu@3 {
 			device_type = "cpu";
 			compatible = "arm,cortex-a7";
-			enable-method = "qcom,kpss-acc-v1";
+			enable-method = "qcom,kpss-acc-v2";
+			next-level-cache = <&L2>;
 			qcom,acc = <&acc3>;
 			qcom,saw = <&saw3>;
 			reg = <0x3>;
@@ -236,22 +246,22 @@
 		};
 
                 acc0: clock-controller@b088000 {
-                        compatible = "qcom,kpss-acc-v1";
+                        compatible = "qcom,kpss-acc-v2";
                         reg = <0x0b088000 0x1000>, <0xb008000 0x1000>;
                 };
 
                 acc1: clock-controller@b098000 {
-                        compatible = "qcom,kpss-acc-v1";
+                        compatible = "qcom,kpss-acc-v2";
                         reg = <0x0b098000 0x1000>, <0xb008000 0x1000>;
                 };
 
                 acc2: clock-controller@b0a8000 {
-                        compatible = "qcom,kpss-acc-v1";
+                        compatible = "qcom,kpss-acc-v2";
                         reg = <0x0b0a8000 0x1000>, <0xb008000 0x1000>;
                 };
 
                 acc3: clock-controller@b0b8000 {
-                        compatible = "qcom,kpss-acc-v1";
+                        compatible = "qcom,kpss-acc-v2";
                         reg = <0x0b0b8000 0x1000>, <0xb008000 0x1000>;
                 };
 
@@ -279,6 +289,12 @@
                         regulator;
                 };
 
+		saw_l2: regulator@b012000 {
+			compatible = "qcom,saw2";
+			reg = <0xb012000 0x1000>;
+			regulator;
+		};
+
 		serial@78af000 {
 			compatible = "qcom,msm-uartdm-v1.4", "qcom,msm-uartdm";
 			reg = <0x78af000 0x200>;
