From 5eed0bf3bc3e69b20a13d8ffcdf97cb720391637 Mon Sep 17 00:00:00 2001
From: Russell King <rmk+kernel@arm.linux.org.uk>
Date: Thu, 1 Oct 2015 00:34:08 +0100
Subject: [PATCH 735/744] phy: marvell: 88E1512: add flow control support

The Marvell PHYs support pause frame advertisments, so we should not be
masking their support off.  Add the necessary flag to the Marvell PHY
to allow any MAC level pause frame support to be advertised.

Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Russell King <rmk+kernel@arm.linux.org.uk>
---
 drivers/net/phy/marvell.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/phy/marvell.c
+++ b/drivers/net/phy/marvell.c
@@ -1148,7 +1148,7 @@ static struct phy_driver marvell_drivers
 		.phy_id = MARVELL_PHY_ID_88E1510,
 		.phy_id_mask = MARVELL_PHY_ID_MASK,
 		.name = "Marvell 88E1510",
-		.features = PHY_GBIT_FEATURES,
+		.features = PHY_GBIT_FEATURES | SUPPORTED_Pause,
 		.flags = PHY_HAS_INTERRUPT,
 		.config_aneg = &m88e1510_config_aneg,
 		.read_status = &marvell_read_status,
