From fe29727caa7fe434fcb3166df2a62672bc516b54 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Petr=20=C5=A0tetiar?= <ynezz@true.cz>
Date: Wed, 4 Nov 2015 16:23:37 +0100
Subject: [PATCH 2/2] USB: qmi_wwan: Add quirk for Quectel EC20 Mini PCIe
 module
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This device has same vendor and product IDs as G2K devices, but it has
different number of interfaces(4 vs 5) and also different interface
layout where EC20 has QMI on interface 4 instead of 0.

lsusb output:

	Bus 002 Device 003: ID 05c6:9215 Qualcomm, Inc. Acer Gobi 2000
	Device Descriptor:
	  bLength                18
	  bDescriptorType         1
	  bcdUSB               2.00
	  bDeviceClass            0 (Defined at Interface level)
	  bDeviceSubClass         0
	  bDeviceProtocol         0
	  bMaxPacketSize0        64
	  idVendor           0x05c6 Qualcomm, Inc.
	  idProduct          0x9215 Acer Gobi 2000 Wireless Modem
	  bcdDevice            2.32
	  iManufacturer           1 Quectel
	  iProduct                2 Quectel LTE Module
	  iSerial                 0
	  bNumConfigurations      1
	  Configuration Descriptor:
	    bLength                 9
	    bDescriptorType         2
	    wTotalLength          209
	    bNumInterfaces          5
	    bConfigurationValue     1
	    iConfiguration          0
	    bmAttributes         0xa0
	      (Bus Powered)
	      Remote Wakeup
	    MaxPower              500mA

Signed-off-by: Petr Štetiar <ynezz@true.cz>
---
 drivers/net/usb/qmi_wwan.c |   21 +++++++++++++++++++++
 1 file changed, 21 insertions(+)

--- a/drivers/net/usb/qmi_wwan.c
+++ b/drivers/net/usb/qmi_wwan.c
@@ -822,6 +822,7 @@ static const struct usb_device_id produc
 	{QMI_GOBI_DEVICE(0x05c6, 0x9245)},	/* Samsung Gobi 2000 Modem device (VL176) */
 	{QMI_GOBI_DEVICE(0x03f0, 0x251d)},	/* HP Gobi 2000 Modem device (VP412) */
 	{QMI_GOBI_DEVICE(0x05c6, 0x9215)},	/* Acer Gobi 2000 Modem device (VP413) */
+	{QMI_FIXED_INTF(0x05c6, 0x9215, 4)},	/* Quectel EC20 Mini PCIe */
 	{QMI_GOBI_DEVICE(0x05c6, 0x9265)},	/* Asus Gobi 2000 Modem device (VR305) */
 	{QMI_GOBI_DEVICE(0x05c6, 0x9235)},	/* Top Global Gobi 2000 Modem device (VR306) */
 	{QMI_GOBI_DEVICE(0x05c6, 0x9275)},	/* iRex Technologies Gobi 2000 Modem device (VR307) */
@@ -853,10 +854,24 @@ static const struct usb_device_id produc
 };
 MODULE_DEVICE_TABLE(usb, products);
 
+static bool quectel_ec20_detected(struct usb_interface *intf)
+{
+	struct usb_device *dev = interface_to_usbdev(intf);
+
+	if (dev->actconfig &&
+	    le16_to_cpu(dev->descriptor.idVendor) == 0x05c6 &&
+	    le16_to_cpu(dev->descriptor.idProduct) == 0x9215 &&
+	    dev->actconfig->desc.bNumInterfaces == 5)
+		return true;
+
+	return false;
+}
+
 static int qmi_wwan_probe(struct usb_interface *intf,
 			  const struct usb_device_id *prod)
 {
 	struct usb_device_id *id = (struct usb_device_id *)prod;
+	struct usb_interface_descriptor *desc = &intf->cur_altsetting->desc;
 
 	/* Workaround to enable dynamic IDs.  This disables usbnet
 	 * blacklisting functionality.  Which, if required, can be
@@ -868,6 +883,12 @@ static int qmi_wwan_probe(struct usb_int
 		id->driver_info = (unsigned long)&qmi_wwan_info;
 	}
 
+	/* Quectel EC20 quirk where we've QMI on interface 4 instead of 0 */
+	if (quectel_ec20_detected(intf) && desc->bInterfaceNumber == 0) {
+		dev_dbg(&intf->dev, "Quectel EC20 quirk, skipping interface 0\n");
+		return -ENODEV;
+	}
+
 	return usbnet_probe(intf, id);
 }
 
