/dts-v1/;

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "netgear,wndr3700-v5", "mediatek,mt7621-soc";
	model = "Netgear WNDR3700v5";

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x8000000>;
	};

	chosen {
		bootargs = "console=ttyS0,57600 maxcpus=2";
	};

	gpio-leds {
		compatible = "gpio-leds";

		wps {
			label = "wndr3700v5:green:wps";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		power {
			label = "wndr3700v5:green:power";
			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <20>;

		wps {
			label = "wndr3700v5:wps";
			gpios = <&gpio0 7 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		wifi {
			label = "wndr3700v5:wifi";
			gpios = <&gpio0 8 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RFKILL>;
		};

		reset {
			label = "wndr3700v5:reset";
			gpios = <&gpio0 14 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		usbpower {
			gpio-export,name = "usbpower";
			gpio-export,output = <1>;
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
		};
	};
};

&spi0 {
	status = "okay";

	mx25l12805d@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;
		m25p,chunked-io = <32>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x30000>;
			read-only;
		};

		partition@30000 {
			label = "u-boot-env";
			reg = <0x30000 0x10000>;
			read-only;
		};

		factory: partition@f30000 {
			label = "factory";
			reg = <0xf30000 0x10000>;
			read-only;
		};

		partition@50000 {
			label = "firmware";
			reg = <0x50000 0xee0000>;
		};
	};
};

&pcie {
	status = "okay";

	pcie0 {
		mt76@0,0 {
			reg = <0x0000 0 0 0 0>;
			device_type = "pci";
			mediatek,mtd-eeprom = <&factory 0x8000>;
			ieee80211-freq-limit = <5000000 6000000>;
		};
	};

	pcie1 {
		mt76@1,0 {
			reg = <0x0000 0 0 0 0>;
			device_type = "pci";
			mediatek,mtd-eeprom = <&factory 0x0000>;
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x0000000c>;
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group =  "rgmii2", "mdio", "wdt";
			ralink,function = "gpio";
		};
	};
};
