/dts-v1/;

#include "vr9.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "ASL56026 - BT OpenReach VDSL Modem";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;

		led-dsl = &dsl;
	};

	memory@0 {
		reg = <0x0 0x2000000>;
	};

	fpi@10000000 {
		localbus@0 {
			nor-boot@0 {
				compatible = "lantiq,nor";
				bank-width = <2>;
				reg = <0 0x0 0x0800000>;
				#address-cells = <1>;
				#size-cells = <1>;

				partitions {
					compatible = "fixed-partitions";
					#address-cells = <1>;
					#size-cells = <1>;

					partition@0 {
						label = "uboot";
						reg = <0x0 0x30000>;
					};

					partition@30000 {
						label = "uboot_env";
						reg = <0x30000 0x10000>;
					};

					partition@40000 {
						label = "firmware";
						reg = <0x40000 0x750000>;
					};

					partition@790000 {
						label = "ddrconfig";
						reg = <0x790000 0x70000>;
						read-only;
					};
				};
			};
		};

		gpio: pinmux@E100B10 {
			pinctrl-names = "default";
			pinctrl-0 = <&state_default>;

			state_default: pinmux {
				mdio {
					lantiq,groups = "mdio";
					lantiq,function = "mdio";
				};
			};
		};
	};

	gphy-xrx200 {
		compatible = "lantiq,phy-xrx200";
		firmware1 = "lantiq/vr9_phy22f_a1x.bin";	/*VR9 1.1*/
		firmware2 = "lantiq/vr9_phy22f_a2x.bin";	/*VR9 1.2*/
		phys = [ 00 01 ];
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio 40 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		dsl: dsl {
			label = "asl56026:green:dsl";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
		};

		/* power-* is a bicolour led */
		power_green: power_green {
			label = "asl56026:green:power";
			gpios = <&gpio 17 GPIO_ACTIVE_HIGH>;
			default-state = "keep";
		};

		power_red: power_red {
			label = "asl56026:red:power";
			gpios = <&gpio 18 GPIO_ACTIVE_HIGH>;
		};
	};

	gpio_export {
		compatible = "gpio-export";
		#size-cells = <0>;

		power_led_blink {
			gpio-export,name = "power_led_blink";
			gpio-export,output = <0>;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};
};

&eth0 {
	lan: interface@0 {
		compatible = "lantiq,xrx200-pdi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;
		lantiq,switch;

		ethernet@2 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <2>;
			phy-mode = "mii";
			phy-handle = <&phy11>;
		};

		ethernet@3 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <3>;
			phy-mode = "mii";
			phy-handle = <&phy14>;
		};

	};

	mdio@0 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "lantiq,xrx200-mdio";

		phy11: ethernet-phy@11 {
			reg = <0x11>;
			compatible = "lantiq,phy22f", "ethernet-phy-ieee802.3-c22";
		};

		phy14: ethernet-phy@14 {
			reg = <0x14>;
			compatible = "lantiq,phy22f", "ethernet-phy-ieee802.3-c22";
		};

	};
};
