From f8e3fcf18e1f2d7f9e6a9680c5452da090f33d88 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Thu, 1 Aug 2013 14:40:44 +0200
Subject: [PATCH] rt2x00: rt2800lib: enable VCO calibration for RF3853

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
---
 drivers/net/wireless/ralink/rt2x00/rt2800lib.c |    2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt2800lib.c
@@ -4871,6 +4871,7 @@ void rt2800_vco_calibration(struct rt2x0
 	case RF3053:
 	case RF3070:
 	case RF3290:
+	case RF3853:
 	case RF5350:
 	case RF5360:
 	case RF5362:
@@ -9420,6 +9421,7 @@ static int rt2800_probe_hw_mode(struct r
 	case RF3053:
 	case RF3070:
 	case RF3290:
+	case RF3853:
 	case RF5350:
 	case RF5360:
 	case RF5362:
