From a6ef8db0e46713da43c81bc15fed01a4da0bd5a4 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Fri, 1 Jul 2016 22:09:24 +0100
Subject: [PATCH] spi-bcm2835: Disable forced software CS

Select software CS in bcm2708_common.dtsi, and disable the automatic
conversion in the driver to allow hardware CS to be re-enabled with an
overlay.

See: https://github.com/raspberrypi/linux/issues/1547

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/bcm283x.dtsi | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/arm/boot/dts/bcm283x.dtsi
+++ b/arch/arm/boot/dts/bcm283x.dtsi
@@ -366,6 +366,7 @@
 			#address-cells = <1>;
 			#size-cells = <0>;
 			status = "disabled";
+			cs-gpios = <&gpio 8 1>, <&gpio 7 1>;
 		};
 
 		i2c0: i2c@7e205000 {
