From 5a95e58e58da417ca8a8f4ae11347ad9a66803cd Mon Sep 17 00:00:00 2001
From: Mingkai Hu <mingkai.hu@nxp.com>
Date: Mon, 26 Sep 2016 12:17:36 +0800
Subject: [PATCH 128/141] pci/layerscape: add LS1046A support

commit a52797fe443a79c53d0b63c505c99f65264de8b7
[context adjustment]

Signed-off-by: Mingkai Hu <mingkai.hu@nxp.com>
Integrated-by: Zhao Qiang <qiang.zhao@nxp.com>
Integrated-by: Yutang Jiang <yutang.jiang@nxp.com>
---
 drivers/pci/host/pci-layerscape.c |    7 +++++++
 1 file changed, 7 insertions(+)

--- a/drivers/pci/host/pci-layerscape.c
+++ b/drivers/pci/host/pci-layerscape.c
@@ -205,6 +205,12 @@ static struct ls_pcie_drvdata ls1043_drv
 	.ops = &ls_pcie_host_ops,
 };
 
+static struct ls_pcie_drvdata ls1046_drvdata = {
+	.lut_offset = 0x10000,
+	.ltssm_shift = 24,
+	.ops = &ls_pcie_host_ops,
+};
+
 static struct ls_pcie_drvdata ls2080_drvdata = {
 	.lut_offset = 0x80000,
 	.ltssm_shift = 0,
@@ -215,6 +221,7 @@ static const struct of_device_id ls_pcie
 	{ .compatible = "fsl,ls1012a-pcie", .data = &ls1012_drvdata },
 	{ .compatible = "fsl,ls1021a-pcie", .data = &ls1021_drvdata },
 	{ .compatible = "fsl,ls1043a-pcie", .data = &ls1043_drvdata },
+	{ .compatible = "fsl,ls1046a-pcie", .data = &ls1046_drvdata },
 	{ .compatible = "fsl,ls2080a-pcie", .data = &ls2080_drvdata },
 	{ .compatible = "fsl,ls2085a-pcie", .data = &ls2080_drvdata },
 	{ },
