/dts-v1/;

#include "danube.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "ARV752DPW22 - Arcor 803";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_red;
		led-failsafe = &power_blue;
		led-running = &power_red;

		led-dsl = &internet_red;
		led-usb = &umts;
		led-wifi = &wifi;
	};

	memory@0 {
		reg = <0x0 0x4000000>;
	};

	sram@1F000000 {
		vmmc@107000 {
			status = "okay";
			gpios = <&gpiomm 1 GPIO_ACTIVE_HIGH>;
		};
	};

	fpi@10000000 {
		localbus@0 {
			nor-boot@0 {
				compatible = "lantiq,nor";
				bank-width = <2>;
				reg = <0 0x0 0x800000>;
				#address-cells = <1>;
				#size-cells = <1>;

				partitions {
					compatible = "fixed-partitions";
					#address-cells = <1>;
					#size-cells = <1>;

					partition@0 {
						label = "uboot";
						reg = <0x00000 0x30000>;
						read-only;
					};

					partition@10000 {
						label = "uboot_env";
						reg = <0x30000 0x10000>;
						read-only;
					};

					partition@20000 {
						label = "firmware";
						reg = <0x40000 0x7b0000>;
					};

					boardconfig: partition@7f0000 {
						label = "board_config";
						reg = <0x7f0000 0x10000>;
						read-only;
					};
				};
			};

			gpiomm: gpiomm@4000000 {
				compatible = "lantiq,gpio-mm";
				reg = <1 0x0 0x10 >;
				#address-cells = <1>;
				#size-cells = <1>;
				#gpio-cells = <2>;
				gpio-controller;
				lantiq,shadow = <3>;
			};
		};

		gpio: pinmux@E100B10 {
			pinctrl-names = "default";
			pinctrl-0 = <&state_default>;

			state_default: pinmux {
				ebu {
					lantiq,groups = "ebu cs1";
					lantiq,function = "ebu";
				};
				exin {
					lantiq,groups = "exin1";
					lantiq,function = "exin";
					lantiq,pull = <2>;
					lantiq,output = <0>;
				};
				pci_in {
					lantiq,groups = "req1";
					lantiq,function = "pci";
					lantiq,pull = <2>;
					lantiq,output = <0>;
				};
				pci_out {
					lantiq,groups = "gnt1";
					lantiq,function = "pci";
					lantiq,open-drain = <1>;
					lantiq,output = <1>;
				};
				pci_rst {
					lantiq,pins = "io21";
					lantiq,open-drain = <1>;
					lantiq,output = <1>;
				};
				leds {
					lantiq,pins = "io3", "io5", "io6", "io8";
					lantiq,open-drain = <1>;
					lantiq,output = <1>;
				};
				buttons {
					lantiq,pins = "io11", "io12", "io13", "io28";
					lantiq,pull = <2>;
					lantiq,output = <0>;
				};
			};
		};

		ifxhcd@E101000 {
			status = "okay";
			gpios = <&gpiomm 0 GPIO_ACTIVE_HIGH>;
		};

		etop@E180000 {
			phy-mode = "mii";
			mtd-mac-address = <&boardconfig 0x16>;
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
		restart {
			label = "restart";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
		};
		dsl {
			label = "dsl";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};
		reset {
			label = "reset";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";
		power_blue: power1 {
			label = "arv752dpw22:blue:power";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};
		internet_red: internet {
			label = "arv752dpw22:red:internet";
			gpios = <&gpio 4 GPIO_ACTIVE_LOW>;
		};
		message {
			label = "arv752dpw22:red:message";
			gpios = <&gpio 5 GPIO_ACTIVE_LOW>;
		};
		power_red: power {
			label = "arv752dpw22:red:power";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		voice1 {
			label = "arv752dpw22:red:voice";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};
		umts: umts {
			label = "arv752dpw22:red:umts";
			gpios = <&gpiomm 3 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "arv752dpw22:red:wifi";
			gpios = <&gpiomm 4 GPIO_ACTIVE_LOW>;
		};
		fxs1 {
			label = "arv752dpw22:green:tae-n";
			gpios = <&gpiomm 5 GPIO_ACTIVE_LOW>;
		};
		fxs2 {
			label = "arv752dpw22:green:tae-u";
			gpios = <&gpiomm 6 GPIO_ACTIVE_LOW>;
		};
		fxo {
			label = "arv752dpw22:green:isdn";
			gpios = <&gpiomm 7 GPIO_ACTIVE_LOW>;
		};
		internet2 {
			label = "arv752dpw22:blue:internet";
			gpios = <&gpiomm 8 GPIO_ACTIVE_LOW>;
		};
		voice2 {
			label = "arv752dpw22:blue:voice";
			gpios = <&gpiomm 9 GPIO_ACTIVE_LOW>;
		};
		eth1 {
			 label = "arv752dpw22:green:lan1";
			 gpios = <&gpiomm 11 GPIO_ACTIVE_LOW>;
		};
		eth2 {
			label = "arv752dpw22:green:lan2";
			gpios = <&gpiomm 12 GPIO_ACTIVE_LOW>;
		};
		eth3 {
			label = "arv752dpw22:green:lan3";
			gpios = <&gpiomm 13 GPIO_ACTIVE_LOW>;
		};
		eth4 {
			label = "arv752dpw22:green:lan4";
			gpios = <&gpiomm 14 GPIO_ACTIVE_LOW>;
		};
	};
};

&pci0 {
	status = "okay";
	lantiq,external-clock;
	interrupt-map = <
		0x7000 0 0 1 &icu0 30
		0x7800 0 0 1 &icu0 135
		0x7800 0 0 2 &icu0 135
		0x7800 0 0 3 &icu0 135
	>;
	gpio-reset = <&gpio 21 GPIO_ACTIVE_HIGH>;
	req-mask = <0x3>;

	wifi@1814,3592 {
		compatible = "pci1814,3592";
		reg = <0x7000 0 0 0 0>;
		ralink,mtd-eeprom = <&boardconfig 0x410>;
		ralink,mtd-eeprom-swap;
	};
};
