From: Ben Greear <greearb@candelatech.com>
Date: Wed, 31 May 2017 14:21:21 +0300
Subject: [PATCH] ath10k: log when longer bmi cmds happen

This lets one have a clue that maybe timeouts are happening
when we just aren't waiting long enough.

Signed-off-by: Ben Greear <greearb@candelatech.com>
Signed-off-by: Kalle Valo <kvalo@qca.qualcomm.com>
---

--- a/drivers/net/wireless/ath/ath10k/pci.c
+++ b/drivers/net/wireless/ath/ath10k/pci.c
@@ -101,7 +101,8 @@ static int ath10k_pci_init_irq(struct at
 static int ath10k_pci_deinit_irq(struct ath10k *ar);
 static int ath10k_pci_request_irq(struct ath10k *ar);
 static void ath10k_pci_free_irq(struct ath10k *ar);
-static int ath10k_pci_bmi_wait(struct ath10k_ce_pipe *tx_pipe,
+static int ath10k_pci_bmi_wait(struct ath10k *ar,
+			       struct ath10k_ce_pipe *tx_pipe,
 			       struct ath10k_ce_pipe *rx_pipe,
 			       struct bmi_xfer *xfer);
 static int ath10k_pci_qca99x0_chip_reset(struct ath10k *ar);
@@ -1843,7 +1844,7 @@ int ath10k_pci_hif_exchange_bmi_msg(stru
 	if (ret)
 		goto err_resp;
 
-	ret = ath10k_pci_bmi_wait(ce_tx, ce_rx, &xfer);
+	ret = ath10k_pci_bmi_wait(ar, ce_tx, ce_rx, &xfer);
 	if (ret) {
 		u32 unused_buffer;
 		unsigned int unused_nbytes;
@@ -1910,23 +1911,37 @@ static void ath10k_pci_bmi_recv_data(str
 	xfer->rx_done = true;
 }
 
-static int ath10k_pci_bmi_wait(struct ath10k_ce_pipe *tx_pipe,
+static int ath10k_pci_bmi_wait(struct ath10k *ar,
+			       struct ath10k_ce_pipe *tx_pipe,
 			       struct ath10k_ce_pipe *rx_pipe,
 			       struct bmi_xfer *xfer)
 {
 	unsigned long timeout = jiffies + BMI_COMMUNICATION_TIMEOUT_HZ;
+	unsigned long started = jiffies;
+	unsigned long dur;
+	int ret;
 
 	while (time_before_eq(jiffies, timeout)) {
 		ath10k_pci_bmi_send_done(tx_pipe);
 		ath10k_pci_bmi_recv_data(rx_pipe);
 
-		if (xfer->tx_done && (xfer->rx_done == xfer->wait_for_resp))
-			return 0;
+		if (xfer->tx_done && (xfer->rx_done == xfer->wait_for_resp)) {
+			ret = 0;
+			goto out;
+		}
 
 		schedule();
 	}
 
-	return -ETIMEDOUT;
+	ret = -ETIMEDOUT;
+
+out:
+	dur = jiffies - started;
+	if (dur > HZ)
+		ath10k_dbg(ar, ATH10K_DBG_BMI,
+			   "bmi cmd took %lu jiffies hz %d ret %d\n",
+			   dur, HZ, ret);
+	return ret;
 }
 
 /*
