/dts-v1/;

#include "rt3050.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "huawei,hg255d", "ralink,rt3052-soc";
	model = "HuaWei HG255D";

	cfi@1f000000 {
		compatible = "cfi-flash";
		reg = <0x1f000000 0x1000000>;
		bank-width = <2>;
		device-width = <2>;
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x40000>;
			read-only;
		};

		partition@30000 {
			label = "u-boot-env";
			reg = <0x40000 0x20000>;
			read-only;
		};

		factory: partition@60000 {
			label = "factory";
			reg = <0x60000 0x20000>;
			read-only;
		};

		partition@80000 {
			label = "firmware";
			reg = <0x80000 0xf60000>;
		};

		partition@fa0000 {
			label = "factory-orig";
			reg = <0xfa0000 0x20000>;
			read-only;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		power {
			label = "hg255d:green:power";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};

		internet {
			label = "hg255d:green:internet";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};

		wifi {
			label = "hg255d:green:wlan";
			gpios = <&gpio0 14 GPIO_ACTIVE_LOW>;
		};

		usb {
			label = "hg255d:green:usb";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = "hg255d:green:wps";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		voice {
			label = "hg255d:green:voice";
			gpios = <&gpio0 5 GPIO_ACTIVE_LOW>;
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <10>;

		reset {
			label = "reset";
			gpios = <&gpio0 4 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		rfkill {
			label = "rfkill";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};
	};
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "spi", "i2c", "jtag", "rgmii", "mdio", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x28>;
};

&esw {
	mediatek,portmap = <0x2f>;
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};

&otg {
	status = "okay";
};
