--- a/arch/arm/boot/dts/armada-xp-linksys-mamba.dts
+++ b/arch/arm/boot/dts/armada-xp-linksys-mamba.dts
@@ -298,7 +298,6 @@
 			nand@d0000 {
 				status = "okay";
 				num-cs = <1>;
-				marvell,nand-keep-config;
 				marvell,nand-enable-arbiter;
 				nand-on-flash-bbt;
 				nand-ecc-strength = <4>;
