From 60eedf7a9512683e2a8a998863cc5942e9dbdae5 Mon Sep 17 00:00:00 2001
From: Minghuan Lian <Minghuan.Lian@nxp.com>
Date: Tue, 17 Jan 2017 17:32:39 +0800
Subject: [PATCH 08/13] arm64: dts: ls1043a: share all MSIs

Cherry-pick patchwork patch.

In order to maximize the use of MSI, a PCIe controller will share
all MSI controllers. The patch changes "msi-parent" to refer to all
MSI controller dts nodes.

Signed-off-by: Minghuan Lian <Minghuan.Lian@nxp.com>
Signed-off-by: Yangbo Lu <yangbo.lu@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi | 6 +++---
 1 file changed, 3 insertions(+), 3 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
@@ -1033,7 +1033,7 @@
 			bus-range = <0x0 0xff>;
 			ranges = <0x81000000 0x0 0x00000000 0x40 0x00010000 0x0 0x00010000   /* downstream I/O */
 				  0x82000000 0x0 0x40000000 0x40 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&msi1>;
+			msi-parent = <&msi1>, <&msi2>, <&msi3>;
 			#interrupt-cells = <1>;
 			interrupt-map-mask = <0 0 0 7>;
 			interrupt-map = <0000 0 0 1 &gic 0 110 0x4>,
@@ -1058,7 +1058,7 @@
 			bus-range = <0x0 0xff>;
 			ranges = <0x81000000 0x0 0x00000000 0x48 0x00010000 0x0 0x00010000   /* downstream I/O */
 				  0x82000000 0x0 0x40000000 0x48 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&msi2>;
+			msi-parent = <&msi1>, <&msi2>, <&msi3>;
 			#interrupt-cells = <1>;
 			interrupt-map-mask = <0 0 0 7>;
 			interrupt-map = <0000 0 0 1 &gic 0 120  0x4>,
@@ -1083,7 +1083,7 @@
 			bus-range = <0x0 0xff>;
 			ranges = <0x81000000 0x0 0x00000000 0x50 0x00010000 0x0 0x00010000   /* downstream I/O */
 				  0x82000000 0x0 0x40000000 0x50 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
-			msi-parent = <&msi3>;
+			msi-parent = <&msi1>, <&msi2>, <&msi3>;
 			#interrupt-cells = <1>;
 			interrupt-map-mask = <0 0 0 7>;
 			interrupt-map = <0000 0 0 1 &gic 0 154 0x4>,
