From 118d9d4b959d30a582d4bd26d1a1918a43ea0ddf Mon Sep 17 00:00:00 2001
From: Gong Qianyu <Qianyu.Gong@nxp.com>
Date: Wed, 7 Sep 2016 18:33:09 +0800
Subject: [PATCH 13/13] dts: ls1043a: change GIC register for rev1.1

Cherry-pick sdk patch.

Signed-off-by: Gong Qianyu <Qianyu.Gong@nxp.com>
Signed-off-by: Minghuan Lian <Minghuan.Lian@nxp.com>
Signed-off-by: Mingkai Hu <mingkai.hu@nxp.com>
Signed-off-by: Yangbo Lu <yangbo.lu@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi | 8 ++++----
 1 file changed, 4 insertions(+), 4 deletions(-)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
@@ -141,10 +141,10 @@
 		compatible = "arm,gic-400";
 		#interrupt-cells = <3>;
 		interrupt-controller;
-		reg = <0x0 0x1401000 0 0x1000>, /* GICD */
-		      <0x0 0x1402000 0 0x2000>, /* GICC */
-		      <0x0 0x1404000 0 0x2000>, /* GICH */
-		      <0x0 0x1406000 0 0x2000>; /* GICV */
+		reg = <0x0 0x1410000 0 0x10000>, /* GICD */
+		      <0x0 0x1420000 0 0x20000>, /* GICC */
+		      <0x0 0x1440000 0 0x20000>, /* GICH */
+		      <0x0 0x1460000 0 0x20000>; /* GICV */
 		interrupts = <1 9 0xf08>;
 	};
 
