From e555d24e5df9b2d5b8a613ff46af68fc3ff3a360 Mon Sep 17 00:00:00 2001
From: Madalin Bucur <madalin.bucur@freescale.com>
Date: Wed, 30 Mar 2016 16:12:33 +0300
Subject: [PATCH 64/70] dpaa_eth: repair issue introduced with 2.5G support

Signed-off-by: Madalin Bucur <madalin.bucur@freescale.com>
---
 drivers/net/ethernet/freescale/sdk_dpaa/mac.c |    3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

--- a/drivers/net/ethernet/freescale/sdk_dpaa/mac.c
+++ b/drivers/net/ethernet/freescale/sdk_dpaa/mac.c
@@ -346,7 +346,8 @@ static int __cold mac_probe(struct platf
 					SUPPORTED_100baseT_Half);
 
 	/* Gigabit support (no half-duplex) */
-	if (mac_dev->max_speed == 1000)
+	if (mac_dev->max_speed == SPEED_1000 ||
+	    mac_dev->max_speed == SPEED_2500)
 		mac_dev->if_support |= SUPPORTED_1000baseT_Full;
 
 	/* The 10G interface only supports one mode */
