From: Jonas Gorski <jonas.gorski@gmail.com>
Subject: [PATCH] net: bcm63xx_enet: fully reset ephy

Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 drivers/net/ethernet/broadcom/bcm63xx_enet.c |    4 ++--
 1 file changed, 2 insertions(+), , 1 deletions(-)

--- a/drivers/net/ethernet/broadcom/bcm63xx_enet.c
+++ b/drivers/net/ethernet/broadcom/bcm63xx_enet.c
@@ -2857,7 +2857,7 @@ static int bcm_enet_shared_probe(struct
 
 	memset(bcm_enet_shared_base, 0, sizeof(bcm_enet_shared_base));
 
-	ephy_reset = devm_gpiod_get_optional(&pdev->dev, "ephy-reset", GPIOD_ASIS);
+	ephy_reset = devm_gpiod_get_optional(&pdev->dev, "ephy-reset", GPIOD_OUT_HIGH);
 	if (IS_ERR(ephy_reset))
 		return PTR_ERR(ephy_reset);
 
@@ -2871,7 +2871,7 @@ static int bcm_enet_shared_probe(struct
 	memcpy(bcm_enet_shared_base, p, sizeof(bcm_enet_shared_base));
 
 	if (ephy_reset)
-		gpiod_direction_output(ephy_reset, 0);
+		gpiod_set_value(ephy_reset, 0);
 
 	return 0;
 }
