From 9821898bbfa5a21254baafe19b3cc97516fc6019 Mon Sep 17 00:00:00 2001
From: Matthias Brugger <mbrugger@suse.com>
Date: Thu, 14 Apr 2016 23:24:26 +0200
Subject: [PATCH 178/226] staging: fsl-mc: bus: Drop warning

When updating the irq_chip and msi_domain_ops, the code checkes for
already present functions.
When more then one ITS controller are present in the system,
irq_chip and msi_domain_ops got already set and a warning is invoked.

This patch deletes the warning, as the funtions are just already set to
the needed callbacks.

Signed-off-by: Matthias Brugger <mbrugger@suse.com>
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/staging/fsl-mc/bus/mc-msi.c |   12 ++++--------
 1 file changed, 4 insertions(+), 8 deletions(-)

--- a/drivers/staging/fsl-mc/bus/mc-msi.c
+++ b/drivers/staging/fsl-mc/bus/mc-msi.c
@@ -37,10 +37,8 @@ static void fsl_mc_msi_update_dom_ops(st
 	/*
 	 * set_desc should not be set by the caller
 	 */
-	if (WARN_ON(ops->set_desc))
-		return;
-
-	ops->set_desc = fsl_mc_msi_set_desc;
+	if (ops->set_desc == NULL)
+		ops->set_desc = fsl_mc_msi_set_desc;
 }
 
 static void __fsl_mc_msi_write_msg(struct fsl_mc_device *mc_bus_dev,
@@ -129,10 +127,8 @@ static void fsl_mc_msi_update_chip_ops(s
 	/*
 	 * irq_write_msi_msg should not be set by the caller
 	 */
-	if (WARN_ON(chip->irq_write_msi_msg))
-		return;
-
-	chip->irq_write_msi_msg = fsl_mc_msi_write_msg;
+	if (chip->irq_write_msi_msg == NULL)
+		chip->irq_write_msi_msg = fsl_mc_msi_write_msg;
 }
 
 /**
