From 0b660259e927177dc0c6eb3b1c39f23c6a011c5f Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Wed, 8 Mar 2017 07:41:05 +0100
Subject: [PATCH] ARM: dts: BCM5301X: Don't use nonexistent "default-off" LED
 trigger
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Such a trigger doesn't exist in Linux and is not needed as LED is being
turned off by default. This could cause errors in LEDs core code when
trying to set default trigger.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts        |  5 -----
 arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts        |  2 --
 arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts  |  5 -----
 arch/arm/boot/dts/bcm4708-netgear-r6250.dts        |  3 ---
 arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts     |  3 ---
 arch/arm/boot/dts/bcm4708-smartrg-sr400ac.dts      | 10 ----------
 arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts        |  2 --
 arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts |  4 ----
 arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts        |  2 --
 arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts  |  8 --------
 arch/arm/boot/dts/bcm4709-netgear-r7000.dts        |  7 -------
 arch/arm/boot/dts/bcm4709-netgear-r8000.dts        |  9 ---------
 arch/arm/boot/dts/bcm4709-tplink-archer-c9-v1.dts  |  8 --------
 arch/arm/boot/dts/bcm47094-dlink-dir-885l.dts      |  6 ------
 arch/arm/boot/dts/bcm47094-luxul-xwr-3100.dts      |  8 --------
 arch/arm/boot/dts/bcm47094-netgear-r8500.dts       |  6 ------
 16 files changed, 88 deletions(-)

--- a/arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts
+++ b/arch/arm/boot/dts/bcm4708-asus-rt-ac56u.dts
@@ -41,19 +41,16 @@
 		usb3 {
 			label = "bcm53xx:blue:usb3";
 			gpios = <&chipcommon 0 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan {
 			label = "bcm53xx:blue:wan";
 			gpios = <&chipcommon 1 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		lan {
 			label = "bcm53xx:blue:lan";
 			gpios = <&chipcommon 2 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		power {
@@ -71,14 +68,12 @@
 		2ghz {
 			label = "bcm53xx:blue:2ghz";
 			gpios = <&chipcommon 6 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 
 		usb2 {
 			label = "bcm53xx:blue:usb2";
 			gpios = <&chipcommon 14 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts
+++ b/arch/arm/boot/dts/bcm4708-asus-rt-ac68u.dts
@@ -41,7 +41,6 @@
 		usb2 {
 			label = "bcm53xx:blue:usb2";
 			gpios = <&chipcommon 0 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		power {
@@ -59,7 +58,6 @@
 		usb3 {
 			label = "bcm53xx:blue:usb3";
 			gpios = <&chipcommon 14 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts
+++ b/arch/arm/boot/dts/bcm4708-buffalo-wzr-1750dhp.dts
@@ -52,13 +52,11 @@
 		usb {
 			label = "bcm53xx:blue:usb";
 			gpios = <&hc595 0 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		power0 {
 			label = "bcm53xx:red:power";
 			gpios = <&hc595 1 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		power1 {
@@ -76,7 +74,6 @@
 		router1 {
 			label = "bcm53xx:amber:router";
 			gpios = <&hc595 4 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan {
@@ -88,13 +85,11 @@
 		wireless0 {
 			label = "bcm53xx:blue:wireless";
 			gpios = <&hc595 6 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wireless1 {
 			label = "bcm53xx:amber:wireless";
 			gpios = <&hc595 7 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6250.dts
@@ -43,19 +43,16 @@
 		power1 {
 			label = "bcm53xx:amber:power";
 			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb {
 			label = "bcm53xx:blue:usb";
 			gpios = <&chipcommon 8 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		wireless {
 			label = "bcm53xx:blue:wireless";
 			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts
+++ b/arch/arm/boot/dts/bcm4708-netgear-r6300-v2.dts
@@ -47,7 +47,6 @@
 		power0 {
 			label = "bcm53xx:green:power";
 			gpios = <&chipcommon 2 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		power1 {
@@ -59,13 +58,11 @@
 		usb {
 			label = "bcm53xx:blue:usb";
 			gpios = <&chipcommon 8 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		wireless {
 			label = "bcm53xx:blue:wireless";
 			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4708-smartrg-sr400ac.dts
+++ b/arch/arm/boot/dts/bcm4708-smartrg-sr400ac.dts
@@ -37,61 +37,51 @@
 		power-amber {
 			label = "bcm53xx:amber:power";
 			gpios = <&chipcommon 2 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb2 {
 			label = "bcm53xx:white:usb2";
 			gpios = <&chipcommon 3 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb3-white {
 			label = "bcm53xx:white:usb3";
 			gpios = <&chipcommon 4 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb3-green {
 			label = "bcm53xx:green:usb3";
 			gpios = <&chipcommon 5 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wps {
 			label = "bcm53xx:white:wps";
 			gpios = <&chipcommon 6 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		status-red {
 			label = "bcm53xx:red:status";
 			gpios = <&chipcommon 8 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		status-green {
 			label = "bcm53xx:green:status";
 			gpios = <&chipcommon 9 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		status-blue {
 			label = "bcm53xx:blue:status";
 			gpios = <&chipcommon 10 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan-white {
 			label = "bcm53xx:white:wan";
 			gpios = <&chipcommon 12 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan-red {
 			label = "bcm53xx:red:wan";
 			gpios = <&chipcommon 13 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
+++ b/arch/arm/boot/dts/bcm47081-asus-rt-n18u.dts
@@ -47,7 +47,6 @@
 		usb2 {
 			label = "bcm53xx:blue:usb2";
 			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan {
@@ -65,7 +64,6 @@
 		usb3 {
 			label = "bcm53xx:blue:usb3";
 			gpios = <&chipcommon 14 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts
+++ b/arch/arm/boot/dts/bcm47081-buffalo-wzr-600dhp2.dts
@@ -68,7 +68,6 @@
 		power1 {
 			label = "bcm53xx:red:power";
 			gpios = <&hc595 2 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		router0 {
@@ -80,7 +79,6 @@
 		router1 {
 			label = "bcm53xx:amber:router";
 			gpios = <&hc595 4 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan {
@@ -92,13 +90,11 @@
 		wireless0 {
 			label = "bcm53xx:green:wireless";
 			gpios = <&hc595 6 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wireless1 {
 			label = "bcm53xx:amber:wireless";
 			gpios = <&hc595 7 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts
+++ b/arch/arm/boot/dts/bcm4709-asus-rt-ac87u.dts
@@ -41,7 +41,6 @@
 		wps {
 			label = "bcm53xx:blue:wps";
 			gpios = <&chipcommon 1 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		power {
@@ -53,7 +52,6 @@
 		wan {
 			label = "bcm53xx:red:wan";
 			gpios = <&chipcommon 5 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
+++ b/arch/arm/boot/dts/bcm4709-buffalo-wxr-1900dhp.dts
@@ -31,13 +31,11 @@
 		usb {
 			label = "bcm53xx:green:usb";
 			gpios = <&chipcommon 4 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		power-amber {
 			label = "bcm53xx:amber:power";
 			gpios = <&chipcommon 5 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		power-white {
@@ -49,37 +47,31 @@
 		router-amber {
 			label = "bcm53xx:amber:router";
 			gpios = <&chipcommon 7 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		router-white {
 			label = "bcm53xx:white:router";
 			gpios = <&chipcommon 8 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan-amber {
 			label = "bcm53xx:amber:wan";
 			gpios = <&chipcommon 9 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan-white {
 			label = "bcm53xx:white:wan";
 			gpios = <&chipcommon 10 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wireless-amber {
 			label = "bcm53xx:amber:wireless";
 			gpios = <&chipcommon 11 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wireless-white {
 			label = "bcm53xx:white:wireless";
 			gpios = <&chipcommon 12 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4709-netgear-r7000.dts
+++ b/arch/arm/boot/dts/bcm4709-netgear-r7000.dts
@@ -47,43 +47,36 @@
 		power-amber {
 			label = "bcm53xx:amber:power";
 			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		5ghz {
 			label = "bcm53xx:white:5ghz";
 			gpios = <&chipcommon 12 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		2ghz {
 			label = "bcm53xx:white:2ghz";
 			gpios = <&chipcommon 13 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		wps {
 			label = "bcm53xx:white:wps";
 			gpios = <&chipcommon 14 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wireless {
 			label = "bcm53xx:white:wireless";
 			gpios = <&chipcommon 15 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb3 {
 			label = "bcm53xx:white:usb3";
 			gpios = <&chipcommon 17 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb2 {
 			label = "bcm53xx:white:usb2";
 			gpios = <&chipcommon 18 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4709-netgear-r8000.dts
+++ b/arch/arm/boot/dts/bcm4709-netgear-r8000.dts
@@ -47,7 +47,6 @@
 		power-amber {
 			label = "bcm53xx:amber:power";
 			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan-white {
@@ -59,49 +58,41 @@
 		wan-amber {
 			label = "bcm53xx:amber:wan";
 			gpios = <&chipcommon 9 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		5ghz-1 {
 			label = "bcm53xx:white:5ghz-1";
 			gpios = <&chipcommon 12 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		2ghz {
 			label = "bcm53xx:white:2ghz";
 			gpios = <&chipcommon 13 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		wireless {
 			label = "bcm53xx:white:wireless";
 			gpios = <&chipcommon 14 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wps {
 			label = "bcm53xx:white:wps";
 			gpios = <&chipcommon 15 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		5ghz-2 {
 			label = "bcm53xx:white:5ghz-2";
 			gpios = <&chipcommon 16 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb3 {
 			label = "bcm53xx:white:usb3";
 			gpios = <&chipcommon 17 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb2 {
 			label = "bcm53xx:white:usb2";
 			gpios = <&chipcommon 18 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm4709-tplink-archer-c9-v1.dts
+++ b/arch/arm/boot/dts/bcm4709-tplink-archer-c9-v1.dts
@@ -26,49 +26,41 @@
 		lan {
 			label = "bcm53xx:blue:lan";
 			gpios = <&chipcommon 1 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wps {
 			label = "bcm53xx:blue:wps";
 			gpios = <&chipcommon 2 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		2ghz {
 			label = "bcm53xx:blue:2ghz";
 			gpios = <&chipcommon 4 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		5ghz {
 			label = "bcm53xx:blue:5ghz";
 			gpios = <&chipcommon 5 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb3 {
 			label = "bcm53xx:blue:usb3";
 			gpios = <&chipcommon 6 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb2 {
 			label = "bcm53xx:blue:usb2";
 			gpios = <&chipcommon 7 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan-blue {
 			label = "bcm53xx:blue:wan";
 			gpios = <&chipcommon 14 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan-amber {
 			label = "bcm53xx:amber:wan";
 			gpios = <&chipcommon 15 GPIO_ACTIVE_HIGH>;
-			linux,default-trigger = "default-off";
 		};
 
 		power {
--- a/arch/arm/boot/dts/bcm47094-dlink-dir-885l.dts
+++ b/arch/arm/boot/dts/bcm47094-dlink-dir-885l.dts
@@ -56,37 +56,31 @@
 		wan-white {
 			label = "bcm53xx:white:wan";
 			gpios = <&chipcommon 1 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		power-amber {
 			label = "bcm53xx:amber:power";
 			gpios = <&chipcommon 2 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan-amber {
 			label = "bcm53xx:amber:wan";
 			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb3-white {
 			label = "bcm53xx:white:usb3";
 			gpios = <&chipcommon 8 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		2ghz {
 			label = "bcm53xx:white:2ghz";
 			gpios = <&chipcommon 13 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		5ghz {
 			label = "bcm53xx:white:5ghz";
 			gpios = <&chipcommon 14 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm47094-luxul-xwr-3100.dts
+++ b/arch/arm/boot/dts/bcm47094-luxul-xwr-3100.dts
@@ -34,37 +34,31 @@
 		lan3	{
 			label = "bcm53xx:green:lan3";
 			gpios = <&chipcommon 1 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		lan4	{
 			label = "bcm53xx:green:lan4";
 			gpios = <&chipcommon 2 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		wan	{
 			label = "bcm53xx:green:wan";
 			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		lan1	{
 			label = "bcm53xx:green:lan1";
 			gpios = <&chipcommon 4 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		lan2	{
 			label = "bcm53xx:green:lan2";
 			gpios = <&chipcommon 6 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb3	{
 			label = "bcm53xx:green:usb3";
 			gpios = <&chipcommon 8 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		status	{
@@ -76,13 +70,11 @@
 		2ghz {
 			label = "bcm53xx:green:2ghz";
 			gpios = <&chipcommon 13 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		5ghz {
 			label = "bcm53xx:green:5ghz";
 			gpios = <&chipcommon 14 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
--- a/arch/arm/boot/dts/bcm47094-netgear-r8500.dts
+++ b/arch/arm/boot/dts/bcm47094-netgear-r8500.dts
@@ -34,37 +34,31 @@
 		power1 {
 			label = "bcm53xx:amber:power";
 			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		5ghz-1 {
 			label = "bcm53xx:white:5ghz-1";
 			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		5ghz-2 {
 			label = "bcm53xx:white:5ghz-2";
 			gpios = <&chipcommon 12 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		2ghz {
 			label = "bcm53xx:white:2ghz";
 			gpios = <&chipcommon 13 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb2 {
 			label = "bcm53xx:white:usb2";
 			gpios = <&chipcommon 17 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 
 		usb3 {
 			label = "bcm53xx:white:usb3";
 			gpios = <&chipcommon 18 GPIO_ACTIVE_LOW>;
-			linux,default-trigger = "default-off";
 		};
 	};
 
