From d6661da842bbeec2082b7263c9e682792e7951a9 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Tue, 14 Mar 2017 11:39:41 +0100
Subject: [PATCH] ARM: dts: BCM5301X: Add support for TP-LINK Archer C5 V2
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This is BCM47081A0 based home router with BCM43217 and BCM4352 wireless
chipsets.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/Makefile                         |  1 +
 arch/arm/boot/dts/bcm47081-tplink-archer-c5-v2.dts | 98 ++++++++++++++++++++++
 2 files changed, 99 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm47081-tplink-archer-c5-v2.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -86,6 +86,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm47081-buffalo-wzr-900dhp.dtb \
 	bcm47081-luxul-xap-1410.dtb \
 	bcm47081-luxul-xwr-1200.dtb \
+	bcm47081-tplink-archer-c5-v2.dtb \
 	bcm4709-asus-rt-ac87u.dtb \
 	bcm4709-buffalo-wxr-1900dhp.dtb \
 	bcm4709-linksys-ea9200.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/bcm47081-tplink-archer-c5-v2.dts
@@ -0,0 +1,98 @@
+/*
+ * Copyright (C) 2017 Rafał Miłecki <rafal@milecki.pl>
+ *
+ * Licensed under the ISC license.
+ */
+
+/dts-v1/;
+
+#include "bcm47081.dtsi"
+
+/ {
+	compatible = "tplink,archer-c5-v2", "brcm,bcm47081", "brcm,bcm4708";
+	model = "TP-LINK Archer C5 V2";
+
+	chosen {
+		bootargs = "earlycon";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		2ghz {
+			label = "bcm53xx:green:2ghz";
+			gpios = <&chipcommon 0 GPIO_ACTIVE_HIGH>;
+		};
+
+		lan {
+			label = "bcm53xx:green:lan";
+			gpios = <&chipcommon 1 GPIO_ACTIVE_HIGH>;
+		};
+
+		usb2-port1 {
+			label = "bcm53xx:green:usb2-port1";
+			gpios = <&chipcommon 2 GPIO_ACTIVE_HIGH>;
+		};
+
+		power {
+			label = "bcm53xx:green:power";
+			gpios = <&chipcommon 4 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "default-on";
+		};
+
+		wan-green {
+			label = "bcm53xx:green:wan";
+			gpios = <&chipcommon 5 GPIO_ACTIVE_HIGH>;
+		};
+
+		wps {
+			label = "bcm53xx:green:wps";
+			gpios = <&chipcommon 6 GPIO_ACTIVE_HIGH>;
+		};
+
+		wan-amber {
+			label = "bcm53xx:amber:wan";
+			gpios = <&chipcommon 8 GPIO_ACTIVE_HIGH>;
+		};
+
+		5ghz {
+			label = "bcm53xx:green:5ghz";
+			gpios = <&chipcommon 12 GPIO_ACTIVE_HIGH>;
+		};
+
+		usb2-port2 {
+			label = "bcm53xx:green:usb2-port2";
+			gpios = <&chipcommon 13 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		rfkill {
+			label = "WiFi";
+			linux,code = <KEY_RFKILL>;
+			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
+		};
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 7 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&spi_nor {
+	status = "okay";
+};
+
+&usb2 {
+	vcc-gpio = <&chipcommon 9 GPIO_ACTIVE_HIGH>;
+};
