From d4ca73591916b760478d2b04334d5dcadc028e9c Mon Sep 17 00:00:00 2001
From: Eric Dumazet <edumazet@google.com>
Date: Wed, 19 Apr 2017 09:59:24 -0700
Subject: [PATCH] lan78xx: use skb_cow_head() to deal with cloned skbs

We need to ensure there is enough headroom to push extra header,
but we also need to check if we are allowed to change headers.

skb_cow_head() is the proper helper to deal with this.

Fixes: 55d7de9de6c3 ("Microchip's LAN7800 family USB 2/3 to 10/100/1000 Ethernet device driver")
Signed-off-by: Eric Dumazet <edumazet@google.com>
Cc: James Hughes <james.hughes@raspberrypi.org>
Cc: Woojung Huh <woojung.huh@microchip.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/usb/lan78xx.c | 9 ++-------
 1 file changed, 2 insertions(+), 7 deletions(-)

--- a/drivers/net/usb/lan78xx.c
+++ b/drivers/net/usb/lan78xx.c
@@ -2419,14 +2419,9 @@ static struct sk_buff *lan78xx_tx_prep(s
 {
 	u32 tx_cmd_a, tx_cmd_b;
 
-	if (skb_headroom(skb) < TX_OVERHEAD) {
-		struct sk_buff *skb2;
-
-		skb2 = skb_copy_expand(skb, TX_OVERHEAD, 0, flags);
+	if (skb_cow_head(skb, TX_OVERHEAD)) {
 		dev_kfree_skb_any(skb);
-		skb = skb2;
-		if (!skb)
-			return NULL;
+		return NULL;
 	}
 
 	if (lan78xx_linearize(skb) < 0)
