#!/bin/sh
#
# Copyright (C) 2014-2016 OpenWrt.org
# Copyright (C) 2016 LEDE-Project.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
armada-385-linksys-caiman|\
armada-385-linksys-cobra|\
armada-385-linksys-rango|\
armada-385-linksys-shelby|\
armada-xp-linksys-mamba)
	ucidef_set_interfaces_lan_wan "eth0.1" "eth1.2"
	ucidef_add_switch "switch0" \
		"0:lan:4" "1:lan:3" "2:lan:2" "3:lan:1" "5@eth0" "4:wan" "6@eth1"
	;;
armada-385-db-ap)
	ucidef_set_interfaces_lan_wan "eth0 eth1" "eth2"
	;;
armada-xp-gp)
	ucidef_set_interface_lan "eth0 eth1 eth2 eth3"
	;;
armada-388-clearfog-*)
	# eth0 is standalone ethernet
	# eth1 is switch (-pro) or standalone ethernet (-base)
	# eth2 is SFP
	ucidef_set_interfaces_lan_wan "eth1" "eth0 eth2"

	# if switch exists (clearfog-pro)
	# switch port 5 is connected to eth1
	swconfig list 2>&1 | grep -q switch0 && \
		ucidef_add_switch "switch0" \
			"0:lan:5" "1:lan:4" "2:lan:3" "3:lan:2" "4:lan:1" "5u@eth1" "6:lan:6"
	;;
*)
	ucidef_set_interface_lan "eth0"
	;;
esac

board_config_flush

exit 0
