From 81c67bb120106c4fbd9b7191ab057b48e13e3e5e Mon Sep 17 00:00:00 2001
From: Yutang Jiang <yutang.jiang@nxp.com>
Date: Tue, 8 Nov 2016 01:27:50 +0800
Subject: [PATCH 142/142] drivers/mmc: Add compatible string for LS1046A

Signed-off-by: Yutang Jiang <yutang.jiang@nxp.com>
---
 drivers/mmc/host/sdhci-of-esdhc.c |    1 +
 1 file changed, 1 insertion(+)

--- a/drivers/mmc/host/sdhci-of-esdhc.c
+++ b/drivers/mmc/host/sdhci-of-esdhc.c
@@ -607,6 +607,7 @@ static int sdhci_esdhc_probe(struct plat
 	    of_device_is_compatible(np, "fsl,p4080-esdhc") ||
 	    of_device_is_compatible(np, "fsl,p1020-esdhc") ||
 	    of_device_is_compatible(np, "fsl,t1040-esdhc") ||
+		of_device_is_compatible(np, "fsl,ls1046a-esdhc") ||
 	    of_device_is_compatible(np, "fsl,ls1021a-esdhc"))
 		host->quirks &= ~SDHCI_QUIRK_BROKEN_CARD_DETECTION;
 
