From 9c7d787508be6d68a6ec66de3c3466b24e820c71 Mon Sep 17 00:00:00 2001
From: Brian Norris <computersforpeace@gmail.com>
Date: Fri, 30 Oct 2015 20:33:24 -0700
Subject: [PATCH] mtd: spi-nor: convert to spi_nor_{get, set}_flash_node()

Used semantic patch with 'make coccicheck MODE=patch COCCI=script.cocci':

---8<----
virtual patch

@@
struct spi_nor b;
struct spi_nor *c;
expression d;
@@
(
-(b).flash_node = (d)
+spi_nor_set_flash_node(&b, d)
|
-(c)->flash_node = (d)
+spi_nor_set_flash_node(c, d)
)
---8<----

And a manual conversion for the one use of spi_nor_get_flash_node().

Signed-off-by: Brian Norris <computersforpeace@gmail.com>
Reviewed-by: Boris Brezillon <boris.brezillon@free-electrons.com>
---
 drivers/mtd/devices/m25p80.c      | 2 +-
 drivers/mtd/spi-nor/fsl-quadspi.c | 2 +-
 drivers/mtd/spi-nor/nxp-spifi.c   | 2 +-
 drivers/mtd/spi-nor/spi-nor.c     | 2 +-
 4 files changed, 4 insertions(+), 4 deletions(-)

--- a/drivers/mtd/devices/m25p80.c
+++ b/drivers/mtd/devices/m25p80.c
@@ -221,7 +221,7 @@ static int m25p_probe(struct spi_device
 	nor->read_reg = m25p80_read_reg;
 
 	nor->dev = &spi->dev;
-	nor->flash_node = spi->dev.of_node;
+	spi_nor_set_flash_node(nor, spi->dev.of_node);
 	nor->priv = flash;
 
 	spi_set_drvdata(spi, flash);
--- a/drivers/mtd/spi-nor/fsl-quadspi.c
+++ b/drivers/mtd/spi-nor/fsl-quadspi.c
@@ -1013,7 +1013,7 @@ static int fsl_qspi_probe(struct platfor
 		mtd = &nor->mtd;
 
 		nor->dev = dev;
-		nor->flash_node = np;
+		spi_nor_set_flash_node(nor, np);
 		nor->priv = q;
 
 		/* fill the hooks */
--- a/drivers/mtd/spi-nor/nxp-spifi.c
+++ b/drivers/mtd/spi-nor/nxp-spifi.c
@@ -330,7 +330,7 @@ static int nxp_spifi_setup_flash(struct
 	writel(ctrl, spifi->io_base + SPIFI_CTRL);
 
 	spifi->nor.dev   = spifi->dev;
-	spifi->nor.flash_node = np;
+	spi_nor_set_flash_node(&spifi->nor, np);
 	spifi->nor.priv  = spifi;
 	spifi->nor.read  = nxp_spifi_read;
 	spifi->nor.write = nxp_spifi_write;
--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -1120,7 +1120,7 @@ int spi_nor_scan(struct spi_nor *nor, co
 	const struct flash_info *info = NULL;
 	struct device *dev = nor->dev;
 	struct mtd_info *mtd = &nor->mtd;
-	struct device_node *np = nor->flash_node;
+	struct device_node *np = spi_nor_get_flash_node(nor);
 	int ret;
 	int i;
 
