/dts-v1/;

#include "vr9.dtsi"

#include <dt-bindings/input/input.h>

/ {
	model = "FRITZ7360SL - 1&1 HomeServer";

	chosen {
		bootargs = "console=ttyLTQ0,115200";
	};

	aliases {
		led-boot = &power_green;
		led-failsafe = &power_red;
		led-running = &power_green;

		led-dsl = &info_green;
		led-wifi = &wifi;
	};

	memory@0 {
		reg = <0x0 0x8000000>;
	};

	fpi@10000000 {
		localbus@0 {
			nor-boot@0 {
				compatible = "lantiq,nor";
				bank-width = <2>;
				reg = <0 0x0 0x1000000>;
				#address-cells = <1>;
				#size-cells = <1>;
				partitions {
					compatible = "fixed-partitions";
					#address-cells = <1>;
					#size-cells = <1>;
					urlader: partition@0 {
						label = "urlader";
						reg = <0x00000 0x20000>;
						read-only;
					};

					partition@20000 {
						label = "firmware";
						reg = <0x20000 0xf60000>;
					};

					partition@f80000 {
						label = "tffs (1)";
						reg = <0xf80000 0x40000>;
						read-only;
					};

					partition@fc0000 {
						label = "tffs (2)";
						reg = <0xfc0000 0x40000>;
						read-only;
					};
				};
			};
		};

		gpio: pinmux@E100B10 {
			pinctrl-names = "default";
			pinctrl-0 = <&state_default>;

			state_default: pinmux {
				mdio {
					lantiq,groups = "mdio";
					lantiq,function = "mdio";
				};
				phy-rst {
					lantiq,pins = "io37", "io44";
					lantiq,pull = <0>;
					lantiq,open-drain;
					lantiq,output = <1>;
				};
				pcie-rst {
					lantiq,pins = "io38";
					lantiq,pull = <0>;
					lantiq,output = <1>;
				};
			};
		};

		ifxhcd@E101000 {
			status = "okay";
			lantiq,portmask = <0x3>;
		};

		ifxhcd@E106000 {
			status = "okay";
		};
	};

	gphy-xrx200 {
		compatible = "lantiq,phy-xrx200";
		firmware = "lantiq/vr9_phy11g_a2x.bin";
		phys = [ 00 01 ];
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;
		dect {
			label = "dect";
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_PHONE>;
		};
		wifi {
			label = "wifi";
			gpios = <&gpio 29 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_WLAN>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		power_green: power {
			label = "fritz7360sl:green:power";
			gpios = <&gpio 32 GPIO_ACTIVE_LOW>;
			default-state = "keep";
		};
		power_red: power2 {
			label = "fritz7360sl:red:power";
			gpios = <&gpio 33 GPIO_ACTIVE_LOW>;
		};
		info_red {
			label = "fritz7360sl:red:info";
			gpios = <&gpio 34 GPIO_ACTIVE_LOW>;
		};
		info_green: info_green {
			label = "fritz7360sl:green:info";
			gpios = <&gpio 47 GPIO_ACTIVE_LOW>;
		};
		wifi: wifi {
			label = "fritz7360sl:green:wlan";
			gpios = <&gpio 36 GPIO_ACTIVE_LOW>;
		};
		dect {
			label = "fritz7360sl:green:dect";
			gpios = <&gpio 35 GPIO_ACTIVE_LOW>;
		};
	};
};

&eth0 {
	lan: interface@0 {
		compatible = "lantiq,xrx200-pdi";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;
		mtd-mac-address = <&urlader 0xa91>;
		mtd-mac-address-increment = <(-2)>;
		lantiq,switch;

		ethernet@0 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <0>;
			phy-mode = "rmii";
			phy-handle = <&phy0>;
		};
		ethernet@1 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <1>;
			phy-mode = "rmii";
			phy-handle = <&phy1>;
		};
		ethernet@2 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <2>;
			phy-mode = "gmii";
			phy-handle = <&phy11>;
		};
		ethernet@3 {
			compatible = "lantiq,xrx200-pdi-port";
			reg = <4>;
			phy-mode = "gmii";
			phy-handle = <&phy13>;
		};
	};

	mdio@0 {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "lantiq,xrx200-mdio";
		phy0: ethernet-phy@0 {
			reg = <0x00>;
			compatible = "ethernet-phy-id004d.d076", "ethernet-phy-ieee802.3-c22";
			reset-gpios = <&gpio 37 GPIO_ACTIVE_LOW>;
		};
		phy1: ethernet-phy@1 {
			reg = <0x01>;
			compatible = "ethernet-phy-id004d.d076", "ethernet-phy-ieee802.3-c22";
			reset-gpios = <&gpio 44 GPIO_ACTIVE_LOW>;
		};
		phy11: ethernet-phy@11 {
			reg = <0x11>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
		phy13: ethernet-phy@13 {
			reg = <0x13>;
			compatible = "lantiq,phy11g", "ethernet-phy-ieee802.3-c22";
		};
	};
};

&pcie0 {
	pcie@0 {
		reg = <0 0 0 0 0>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		device_type = "pci";

		wifi@168c,002e {
			compatible = "pci168c,002e";
			reg = <0 0 0 0 0>;
			qca,no-eeprom; /* load from ath9k-eeprom-pci-0000:01:00.0.bin */
		};
	};
};
