# Standard Boot-Script
# use only well-known variable names provided by U-Boot Distro boot
# This script assumes that there is a boot partition, 
# and that the root partition is always the next one.

# Override DeviceTree for Clearfog Base
# removed once U-Boot is able to detect the board variant.
setenv fdtfile armada-388-clearfog-base.dtb

# generate bootargs for rootfs on MMC
if test "${devtype}" = "mmc"; then
	setexpr lede_rootpart ${distro_bootpart} + 1
	setenv bootargs ${bootargs} root=/dev/mmcblk${devnum}p${lede_rootpart} rootfstype=auto rootwait
fi

# here one could add logic for other rootfs device types such as scsi and usb

# add console= option to bootargs, if any
if test -n "${console}"; then
	setenv bootargs ${bootargs} console=${console}
fi

echo "Booting Linux with ${bootargs}"
load ${devtype} ${devnum}:${distro_bootpart} ${fdt_addr_r} ${fdtfile}
load ${devtype} ${devnum}:${distro_bootpart} ${kernel_addr_r} zImage
bootz ${kernel_addr_r} - ${fdt_addr_r}
