/dts-v1/;

#include "rt2880.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "dlink,dap-1522-a1", "ralink,rt2880-soc";
	model = "D-Link DAP-1522 A1";

	aliases {
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	cfi@bc400000 {
		compatible = "cfi-flash";
		reg = <0xbc400000 0x800000>;
		bank-width = <2>;
		device-width = <2>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "uboot";
				reg = <0x0 0x30000>;
				read-only;
			};

			factory: partition@30000 {
				label = "factory";
				reg = <0x30000 0x10000>;
				read-only;
			};

			partition@40000 {
				label = "firmware";
				reg = <0x40000 0x3a0000>;
			};
		};
	};

	rtl8366s {
		compatible = "realtek,rtl8366s";
		gpio-sda = <&gpio0 1 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio0 2 GPIO_ACTIVE_HIGH>;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio2 16 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		ap {
			label = "ap";
			gpios = <&gpio2 13 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
			linux,input-type = <EV_SW>;
		};

		bridge {
			label = "bridge";
			gpios = <&gpio2 14 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
			linux,input-type = <EV_SW>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		wps {
			label = "dap-1522-a1:blue:wps";
			gpios = <&gpio2 17 GPIO_ACTIVE_LOW>;
		};

		ap {
			label = "dap-1522-a1:blue:ap";
			gpios = <&gpio2 18 GPIO_ACTIVE_LOW>;
		};

		sta {
			label = "dap-1522-a1:red:sta";
			gpios = <&gpio2 19 GPIO_ACTIVE_LOW>;
		};

		led_status: status {
			label = "dap-1522-a1:blue:status";
			gpios = <&gpio2 20 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio0 {
	status = "okay";
};

&gpio2 {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "uartlite", "pci";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	status = "okay";
	mtd-mac-address = <&factory 0x2004>;

	port@0 {
		mediatek,fixed-link = <1000 1 1 1>;
	};

	mdio-bus {
		status = "okay";

		phy0: ethernet-phy@0 {
			phy-mode = "mii";
			reg = <0>;
		};
	};
};

&wmac {
	ralink,mtd-eeprom = <&factory 0x2000>;
};
