From: Simon Farnsworth <simon@farnz.org.uk>
Date: Sun, 1 Mar 2015 10:54:39 +0000
Subject: [PATCH] pppoe: Use workqueue to die properly when a PADT is received

When a PADT frame is received, the socket may not be in a good state to
close down the PPP interface. The current implementation handles this by
simply blocking all further PPP traffic, and hoping that the lack of traffic
will trigger the user to investigate.

Use schedule_work to get to a process context from which we clear down the
PPP interface, in a fashion analogous to hangup on a TTY-based PPP
interface. This causes pppd to disconnect immediately, and allows tools to
take immediate corrective action.

Note that pppd's rp_pppoe.so plugin has code in it to disable the session
when it disconnects; however, as a consequence of this patch, the session is
already disabled before rp_pppoe.so is asked to disable the session. The
result is a harmless error message:

Failed to disconnect PPPoE socket: 114 Operation already in progress

This message is safe to ignore, as long as the error is 114 Operation
already in progress; in that specific case, it means that the PPPoE session
has already been disabled before pppd tried to disable it.

Signed-off-by: Simon Farnsworth <simon@farnz.org.uk>
Tested-by: Dan Williams <dcbw@redhat.com>
Tested-by: Christoph Schulz <develop@kristov.de>
Signed-off-by: David S. Miller <davem@davemloft.net>
---

--- a/drivers/net/ppp/pppoe.c
+++ b/drivers/net/ppp/pppoe.c
@@ -454,6 +454,18 @@ out:
 	return NET_RX_DROP;
 }
 
+static void pppoe_unbind_sock_work(struct work_struct *work)
+{
+	struct pppox_sock *po = container_of(work, struct pppox_sock,
+					     proto.pppoe.padt_work);
+	struct sock *sk = sk_pppox(po);
+
+	lock_sock(sk);
+	pppox_unbind_sock(sk);
+	release_sock(sk);
+	sock_put(sk);
+}
+
 /************************************************************************
  *
  * Receive a PPPoE Discovery frame.
@@ -499,7 +511,8 @@ static int pppoe_disc_rcv(struct sk_buff
 		}
 
 		bh_unlock_sock(sk);
-		sock_put(sk);
+		if (!schedule_work(&po->proto.pppoe.padt_work))
+			sock_put(sk);
 	}
 
 abort:
@@ -612,6 +625,8 @@ static int pppoe_connect(struct socket *
 
 	lock_sock(sk);
 
+	INIT_WORK(&po->proto.pppoe.padt_work, pppoe_unbind_sock_work);
+
 	error = -EINVAL;
 
 	if (sockaddr_len != sizeof(struct sockaddr_pppox))
--- a/include/linux/if_pppox.h
+++ b/include/linux/if_pppox.h
@@ -19,6 +19,7 @@
 #include <linux/netdevice.h>
 #include <linux/ppp_channel.h>
 #include <linux/skbuff.h>
+#include <linux/workqueue.h>
 #include <uapi/linux/if_pppox.h>
 
 static inline struct pppoe_hdr *pppoe_hdr(const struct sk_buff *skb)
@@ -32,6 +33,7 @@ struct pppoe_opt {
 	struct pppoe_addr	pa;	  /* what this socket is bound to*/
 	struct sockaddr_pppox	relay;	  /* what socket data will be
 					     relayed to (PPPoE relaying) */
+	struct work_struct      padt_work;/* Work item for handling PADT */
 };
 
 struct pptp_opt {
