/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "qca953x.dtsi"

/ {
	aliases {
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-running = &led_status;
		led-upgrade = &led_status;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;
		pinctrl-names = "default";
		pinctrl-0 = <&jtag_disable_pins>;

		button0 {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
		};

		button1 {
			label = "button right";
			linux,code = <BTN_0>;
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
		};

		button3 {
			label = "button left";
			linux,code = <BTN_1>;
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
		};
	};

	leds {
		compatible = "gpio-leds";

		// Colors from non-Lite versions

		led_status: status {
			label = "gl-ar300m:green:status";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};

		led_lan: lan {
			label = "gl-ar300m:green:lan";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
		};

		led_wlan: wlan {
			label = "gl-ar300m:red:wlan";
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};
};

&pcie0 {
	status = "okay";
};

&spi {
	status = "okay";
	num-cs = <0>;

	flash@0 {
		compatible = "winbond,w25q128", "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@1 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			partition@2 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x050000 0xfa0000>;
			};

			art: partition@3 {
				label = "art";
				reg = <0xff0000 0x010000>;
			};
		};
	};
};

&uart {
	status = "okay";
};

&usb0 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&eth0 {
	status = "okay";
	mtd-mac-address = <&art 0x0>;
	phy-handle = <&swphy4>;
};

&eth1 {
	mtd-mac-address = <&art 0x0>;
	mtd-mac-address-increment = <1>;
};

&wmac {
	status = "okay";
	mtd-cal-data = <&art 0x1000>;
	mtd-mac-address = <&art 0x1002>;
};
