#!/bin/sh
# Copyright (C) 2014-2015 OpenWrt.org

. /lib/functions/uci-defaults.sh
. /lib/functions.sh
. /lib/functions/system.sh

board_config_update

board=$(board_name)

case "$board" in
tl-wdr4900-v1)
	ucidef_add_switch "switch0" \
		"0@eth0" "2:lan:1" "3:lan:2" "4:lan:3" "5:lan:4" "1:wan"
	ucidef_set_interface_macaddr "wan" "$(mtd_get_mac_binary config 332)"
	;;
*)
	ucidef_set_interfaces_lan_wan "eth0" "eth1"
	;;
esac

board_config_flush

exit 0
