From 5cbf53c7e5eac5bacc409461888789accdaf8eec Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Thu, 10 Aug 2017 16:00:06 +0200
Subject: [PATCH 51/57] net: mediatek: increase tx_timeout

Signed-off-by: John Crispin <john@phrozen.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -2384,7 +2384,7 @@ static int mtk_add_mac(struct mtk_eth *e
 	mac->hw_stats->reg_offset = id * MTK_STAT_OFFSET;
 
 	SET_NETDEV_DEV(eth->netdev[id], eth->dev);
-	eth->netdev[id]->watchdog_timeo = 5 * HZ;
+	eth->netdev[id]->watchdog_timeo = 30 * HZ;
 	eth->netdev[id]->netdev_ops = &mtk_netdev_ops;
 	eth->netdev[id]->base_addr = (unsigned long)eth->base;
 
