From 99b0e55881b217e9de4efd4d812dd3bd4f8c9380 Mon Sep 17 00:00:00 2001
From: Mingkai Hu <Mingkai.Hu@freescale.com>
Date: Thu, 19 Nov 2015 12:49:50 +0800
Subject: [PATCH 61/70] arm64/layerscape: Enable PCIe for Layerscape

Signed-off-by: Mingkai Hu <Mingkai.Hu@freescale.com>
Integrated-by: Jiang Yutang <yutang.jiang@nxp.com>
---
 arch/arm64/Kconfig.platforms |    2 ++
 1 file changed, 2 insertions(+)

--- a/arch/arm64/Kconfig.platforms
+++ b/arch/arm64/Kconfig.platforms
@@ -31,6 +31,8 @@ config ARCH_EXYNOS7
 
 config ARCH_LAYERSCAPE
 	bool "ARMv8 based Freescale Layerscape SoC family"
+	select PCI_LAYERSCAPE if PCI
+	select LS_SCFG_MSI if PCI_MSI
 	help
 	  This enables support for the Freescale Layerscape SoC family.
 
